**Date Submitted: 10/3/2019**

**Task 00: Execute provided code**

**Youtube Link:**


<https://youtu.be/RNnj99UDnbU>

**------------------------------------------------------------------------------------**

**Task 01:**

Used 67degF instead.

Graph:



Sample 21-36, my hand covered the system to generate some heat.

Youtube Link:

<https://youtu.be/M0nYwIUk_Nk>

**Modified Schematic (if applicable):**

**Modified Code:**

**#include** <stdint.h>

**#include** <stdbool.h>

**#include** "inc/hw\_memmap.h"

**#include** "inc/hw\_types.h"

**#include** "driverlib/debug.h"

**#include** "driverlib/sysctl.h"

**#include** "driverlib/adc.h"

**#include** "driverlib/gpio.h"

**int** **main**(**void**)

{

uint32\_t ui32ADC0Value[4];

**volatile** uint32\_t ui32TempAvg;

**volatile** uint32\_t ui32TempValueC;

**volatile** uint32\_t ui32TempValueF;

**SysCtlClockSet**(SYSCTL\_SYSDIV\_5|SYSCTL\_USE\_PLL|SYSCTL\_OSC\_MAIN|SYSCTL\_XTAL\_16MHZ);

**SysCtlPeripheralEnable**(SYSCTL\_PERIPH\_ADC0);

**ADCSequenceConfigure**(ADC0\_BASE, 2, ADC\_TRIGGER\_PROCESSOR, 0); // Sequencer 2

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 0, ADC\_CTL\_TS);

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 1, ADC\_CTL\_TS);

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 2, ADC\_CTL\_TS);

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 3, ADC\_CTL\_TS|ADC\_CTL\_IE|ADC\_CTL\_END);

**ADCSequenceEnable**(ADC0\_BASE, 2);

// Enable PF1 and PF2 LEDs

**SysCtlPeripheralEnable**(SYSCTL\_PERIPH\_GPIOF);

**GPIOPinTypeGPIOOutput**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2);

**while**(1)

{

**ADCIntClear**(ADC0\_BASE, 2);

**ADCProcessorTrigger**(ADC0\_BASE, 2);

**while**(!**ADCIntStatus**(ADC0\_BASE, 2, **false**))

{

}

**ADCSequenceDataGet**(ADC0\_BASE, 2, ui32ADC0Value);

ui32TempAvg = (ui32ADC0Value[0] + ui32ADC0Value[1] + ui32ADC0Value[2] + ui32ADC0Value[3] + 2)/4;

ui32TempValueC = (1475 - ((2475 \* ui32TempAvg)) / 4096)/10;

ui32TempValueF = ((ui32TempValueC \* 9) + 160) / 5;

// If greater than 67degF change to blue, else red.

**if** (ui32TempValueF > 67)

{

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2, 4);

}

**else**

{

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2, 2);

}


}

}

**------------------------------------------------------------------------------------**

**Task 02:**

Graph:



\*Held down on processor at red marks to generate heat.

Verification:



To find this, I simply turned off the LED after turning it on to check if the timer is working at 0.5s as intended.

Youtube Link:

<https://youtu.be/IXKIg2ZsP6Y>

**Modified Schematic (if applicable):**

**Modified Code:**

**#include** <stdint.h>

**#include** <stdbool.h>

**#include** "inc/tm4c123gh6pm.h"

**#include** "inc/hw\_memmap.h"

**#include** "inc/hw\_types.h"

**#include** "driverlib/debug.h"

**#include** "driverlib/sysctl.h"

**#include** "driverlib/adc.h"

**#include** "driverlib/gpio.h"

**#include** "driverlib/timer.h"

**#include** "driverlib/interrupt.h"

uint32\_t ui32Period;

uint32\_t ui32ADC0Value[4];

**volatile** uint32\_t ui32TempAvg;

**volatile** uint32\_t ui32TempValueC;

**volatile** uint32\_t ui32TempValueF;

**int** **main**(**void**)

{

**SysCtlClockSet**(SYSCTL\_SYSDIV\_5|SYSCTL\_USE\_PLL|SYSCTL\_OSC\_MAIN|SYSCTL\_XTAL\_16MHZ);

**SysCtlPeripheralEnable**(SYSCTL\_PERIPH\_ADC0);

**ADCHardwareOversampleConfigure**(ADC0\_BASE, 32); // Hardware Averaging of 32 Samples

**ADCSequenceConfigure**(ADC0\_BASE, 2, ADC\_TRIGGER\_PROCESSOR, 0); // Sequencer 2

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 0, ADC\_CTL\_TS);

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 1, ADC\_CTL\_TS);

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 2, ADC\_CTL\_TS);

**ADCSequenceStepConfigure**(ADC0\_BASE, 2, 3, ADC\_CTL\_TS|ADC\_CTL\_IE|ADC\_CTL\_END);

// Enable PF1 and PF2 LEDs

**SysCtlPeripheralEnable**(SYSCTL\_PERIPH\_GPIOF);

**GPIOPinTypeGPIOOutput**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2);

**SysCtlPeripheralEnable**(SYSCTL\_PERIPH\_TIMER1);

**TimerConfigure**(TIMER1\_BASE, TIMER\_CFG\_PERIODIC);

ui32Period = **SysCtlClockGet**() / 2;

**TimerLoadSet**(TIMER1\_BASE, TIMER\_A, ui32Period-1);

**IntEnable**(INT\_TIMER1A);

**TimerIntEnable**(TIMER1\_BASE, TIMER\_TIMA\_TIMEOUT);

**IntMasterEnable**();

**TimerEnable**(TIMER1\_BASE, TIMER\_A);

**ADCSequenceEnable**(ADC0\_BASE, 2); // 4 steps \* 32 samples = 128 samples

**ADCIntEnable**(ADC0\_BASE, 2);

**while**(1)

{

}

}

**void** **Timer1AIntHandler**(**void**)

{

**TimerIntClear**(TIMER1\_BASE, TIMER\_A);

**ADCIntClear**(ADC0\_BASE, 2);

**ADCProcessorTrigger**(ADC0\_BASE, 2);

**while**(!**ADCIntStatus**(ADC0\_BASE, 2, **false**))

{

}

**ADCSequenceDataGet**(ADC0\_BASE, 2, ui32ADC0Value);

ui32TempAvg = (ui32ADC0Value[0] + ui32ADC0Value[1] + ui32ADC0Value[2] + ui32ADC0Value[3] + 2)/4;

ui32TempValueC = (1475 - ((2475 \* ui32TempAvg)) / 4096)/10;

ui32TempValueF = ((ui32TempValueC \* 9) + 160) / 5;

// If greater than 67degF change to blue, else red.

**if** (ui32TempValueF > 67)

{

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2, 4);

}

**else**

{

**GPIOPinWrite**(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2, 2);

}

}